00Production Specs | Terms & Conditions | Contact Us | Print Version

Printing: Web offset, perfect bound. Trim Size: 8 %" X 10 %"

Ad Page Dimensions | FEB - MAY 2009 | JUNE - DEC 2009*
NON-BLEED | BLEED | NON-BLEED | BLEED
Full Page | 7 1/4" X 10" | 8 1/2" X 11 1/8" | 7" x 10" | 8-1/4" x 10-3/4"
2/3 Page | 4 5/8" X 10" | 5 3/8" X 11 1/8" | 4-5/8" x 10" | 5-1/4" x 10 3/4"
1/2 Digest | 4 5/8" X 7 5/8" | 5 3/8" X 8 3/8" | 4-5/8" x 7-1/2" | 5-1/4" x 8"
1/2 Horizontal | 7 1/4" X 5" | 8 1/2" X 5 3/8" | 7" x 5" | 8-1/4" x 5-1/4"
1/3 Vertical | 2 1/4" X 10" | 3" X 11 1/8" | 2-1/4" x 10" | 2-7/8" x 10-3/4"
1/3 Square | 4 5/8" X 5" | 5 3/8" X 5 3/8" | 4-5/8" x 5" | 5-1/4" x 5-1/4"
Two-Page Spread | 14 1/2" X 10" | 16 3/4" X 11 1/8" | 14" x 10" | 16-1/4" x 10-3/4"
Spread/Gutter Bleed (only) |  | 15 3/4" X 10" |  | 15-1/4" x 10"

Allow 3/8" safety for live matter from all bleed sides. For spreads, allow 1/4" safety on each side from the gutter.

* As of June 2009 issue new trim size of 8"x10 1/2" will take effect. Please note ad size changes breginning in June 2009 issue.

DIGITAL REQUIREMENTS: Field & Stream utilizes a digital workflow and we require all ad materials be submitted in a digital format. Supplied materials that do not comply with the following specifications will be rejected, or corrected and the advertiser billed for the required production.

AD SIZES: All ads must be created to the exact size specifications on the rate card or will incur charges for re-sizing. All ad files must be supplied with trim and bleed marks. No live copy within 1/4” of gutter or trim on full page or spread ads.

REQUIRED FORMAT: PDF/X-1a is the required file format for all ad submissions. When preparing PDF/X-1a files, careful attention must be paid to insure they are properly created and will reproduce correctly. Please see www.adobe.com/products/acrobat/pdfs/pdfx.pdf for guidelines and instructions. We do not accept application files.

PROOFS: Advertisers must submit a contract-level digital proof at 100% that conforms to SWOP standards (including a color bar) for all ads. To obtain information on acceptable proofs visit the SWOP web site at www.swop.org. Client supplied contract proofs are required in order to guarantee color. Ads without color proofs will be accepted with the understanding that the publisher cannot be held responsible for color reproduction. If a contract proof is not supplied, we will generate an Epson proof at a charge of $42 per page.

MEDIA: CD-ROM, DVD

ELECTRONIC TRANSMISSIONS: If you choose to send your ad files electronically, please contact your Ad Production contact for Bonnier’s FTP login information. For additional information, please visit: http://www.quadarm.com/publisher_sites/main.asp

CONTACTS: Please call in the order listed.
Production Assistant
Shawn Glenn (212) 779-5154
Shawn.Glenn@bonniercorp.com
Production Director
Barbara Taffuri (212) 779-5136
Barbara.Taffuri@bonniercorp.com

SHIPPING INSTRUCTIONS: When shipping ad materials make sure to identify the magazine and issue in which the ad is scheduled to run.
Send All Advertising Materials To:
Attn: Prepress Ad Production
Special Instructions: Magazine/Issue
Bonnier Corporation
460 N. Orlando Ave, Suite 200
Winter Park, FL 32789
1.407.571.4711